
|  |  |  |
| --- | --- | --- |
|  | | |
|  |  |  |

**All Bulk Water Fill Locations**

Effective January 1st, 2020, The Cartier Regional Water Coop no longer supplies a fill hose for water haulers. Customers require their own hose with a 3” Camlock Part C Type fitting to fill. It is also ***mandatory*** that all connections to the system for filling provide an “Airgap”.

**As of September 1, 2020, a warning will be issued for the first offense. If not remediated, on a second infraction your account will be frozen until an “Airgap” is proven to be installed.**

Please refer to the diagram below.



**Please call 204-353-4055 with any questions or concerns**